**Zapytania ofertowe RPO-WG/12 z dnia 20 stycznia 2021 r.**

W dniu 27.01.2021 r. Zamawiający zmienił treść Zapytania ofertowego Opisu przedmiotu zamówienia oraz Formularza ofertowego

Zgodnie z listą zmian:

W wersji polskojęzycznej Opisu przedmiotu zamówienia

Było:

|  |  |  |
| --- | --- | --- |
| **Nazwa towaru** | **Parametry** | **Specyfikacja** |
| **Chłodziarka termoelektryczna**  **2TE na podstawce TO8 12 pin** | przewody zaciskowe AWG30 | Cu czysta miedź cynowana średnica 0,255 mm |
| **Standardowa podstawka TO8** | wysokość pinów poniżej podstawki | 7.8±0.3mm |
| średnica pinów | Ø0.45±0.05 |

Jest:

|  |  |  |
| --- | --- | --- |
| **Nazwa towaru** | **Parametry** | **Specyfikacja** |
| **Chłodziarka termoelektryczna**  **2TE na podstawce TO8 12 pin** | przewody zaciskowe AWG32 | czysta miedź cynowana średnica 0,202 mm |
| **Standardowa podstawka TO8** | wysokość pinów poniżej podstawki | 7.9±0.3mm |
| średnica pinów | Ø0.46±0.05 |

W wersji polskojęzycznej Formularza oferty.

Było:

|  |  |  |  |
| --- | --- | --- | --- |
| **Nazwa towaru** | **Parametry** | **Specyfikacja** | **Tak/Nie** |
| **Chłodziarka termoelektryczna**  **2TE na podstawce TO8 12 pin** | przewody zaciskowe AWG30 | Cu czysta miedź cynowana średnica 0,255 mm |  |
| **Standardowa podstawka TO8** | wysokość pinów poniżej podstawki | 7.8±0.3mm |  |
| średnica pinów | Ø0.45±0.05 |  |

Jest:

|  |  |  |  |
| --- | --- | --- | --- |
| **Nazwa towaru** | **Parametry** | **Specyfikacja** | **Tak/Nie** |
| **Chłodziarka termoelektryczna**  **2TE na podstawce TO8 12 pin** | przewody zaciskowe AWG32 | czysta miedź cynowana średnica 0,202 mm |  |
| **Standardowa podstawka TO8** | wysokość pinów poniżej podstawki | 7.9±0.3mm |  |
| średnica pinów | Ø0.46±0.05 |  |

W wersji polskojęzycznej Zapytania Ofertowego

Punkt 9

Było

**9. Termin składania ofert**

9.1 Ofertę należy złożyć w terminie do **dnia 27 stycznia 2021 r.**

9.2 Wykonawca powinien być związany złożoną ofertą przez okres co najmniej **60 dni**. Bieg terminu związania ofertą rozpoczyna się wraz z upływem terminu składania ofert.

Jest:

**9. Termin składania ofert**

9.1 Ofertę należy złożyć w terminie do **dnia 1 lutego 2021 r.**

9.2 Wykonawca powinien być związany złożoną ofertą przez okres co najmniej **60 dni**. Bieg terminu związania ofertą rozpoczyna się wraz z upływem terminu składania ofert.

Punkt 16

Było:

**16. Postanowienia końcowe**

16.1 Zamawiający zastrzega sobie prawo unieważnienia zapytania ofertowego w każdej chwili, bez podania przyczyny.

16.2 Zamawiający może w każdym czasie bez podania przyczyny odwołać lub zmienić treść niniejszego zapytania ofertowego. Jeżeli zmiany będą miały wpływ na treść ofert składanych w toku postępowania, Zamawiający przedłuży termin składania ofert.

Jest:

**16 Postanowienia końcowe**

16.1 Zamawiający zastrzega sobie prawo unieważnienia zapytania ofertowego w każdej chwili, bez podania przyczyny.

16.2 Zamawiający może w każdym czasie bez podania przyczyny odwołać lub zmienić treść niniejszego zapytania ofertowego. Jeżeli zmiany będą miały wpływ na treść ofert składanych w toku postępowania, Zamawiający przedłuży termin składania ofert.

16.3 Z uwagi na ograniczoną funkcjonalność portalu:

<https://bazakonkurencyjnosci.funduszeeuropejskie.gov.pl/>

Zamawiający wszelkie zmiany dokumentacji Zapytania Ofertowego oraz bieżący, aktualny stan dokumentacji Zapytania Ofertowego będzie publikował na stronie

<https://vigo.com.pl/o-nas/zamowienia/?vigoPublicOrder=25942>

Zamawiający utworzył Zapytanie ofertowe pod tym samym tytułem i numerem.

**Request for proposal No. RPO-WG/12 of January 20, 2021**

On January 20, 2021, the Ordering Party changed the content of the Inquiry

According to the changelog:

In English version of the Order Description

punkt 5.1

Was:

|  |  |  |
| --- | --- | --- |
| **Product name** | **Parametrer** | **Specification** |
| **Thermoelectric cooler 2TE on TO8 12 pin header** | terminal wires  AWG30 | Cu blank tinned copper 0,255  mm dia |
| **Standard**  **TO8 header** | height of the pins below the  header | 7.8±0.3mm |
| diameter of pins | Ø0.45±0.05 |

Is:

|  |  |  |
| --- | --- | --- |
| **Product name** | **Parametrer** | **Specification** |
| **Thermoelectric cooler 2TE on TO8 12 pin header** | terminal wires  AWG32 | blank tinned copper 0,202  mm dia |
| **Standard**  **TO8 header** | height of the pins below the  header | 7.9±0.3mm |
| diameter of pins | Ø0.46±0.05 |

In English version of the Offer from:

Was:

|  |  |  |  |
| --- | --- | --- | --- |
| **Product name** | **Parametrer** | **Specification** | **Yes/No** |
| **Thermoelectric cooler 2TE on TO8 12 pin header** | terminal wires AWG30 | Cu blank tinned copper 0,255  mm dia |  |
| **Standard**  **TO8 header** | height of the pins below the  header | 7.8±0.3mm |  |
| diameter of pins | Ø0.45±0.05 |  |

Is:

|  |  |  |  |
| --- | --- | --- | --- |
| **Product name** | **Parametrer** | **Specification** | **Yes/No** |
| **Thermoelectric cooler 2TE on TO8 12 pin header** | terminal wires  AWG32 | blank tinned copper 0,202  mm dia |  |
| **Standard**  **TO8 header** | height of the  pins below the  header | 7.9±0.3mm |  |
| diameter of  pins | Ø0.46±0.05 |  |

In English version of the Request for proposal:

Point 9:

Was:

**9 Time-limit for submission of tenders**

9.1 The tender should be submitted by:  **January 27, 2021.**

9.2 The Contractor should be bound by the submitted tender for a period of at least **60 days**. The period during which the submitted tender is binding commences at the end of the time limit for submission of tenders.

Is:

**9. Time-limit for submission of tenders**

9.1 The tender should be submitted by:  **February 1, 2021.**

9.2 The Contractor should be bound by the submitted tender for a period of at least **60 days**. The period during which the submitted tender is binding commences at the end of the time limit for submission of tenders.

Point 16

Was:

**16 Final provisions**

16.1The Contracting Party reserves the right to invalidate this request for proposal at any time without providing relevant grounds therefore.

16.2 The Contracting Party may at any time cancel, amend or modify the contents of this request for proposal for convenience. If the amendments or modifications affect the contents of the tenders submitted in the course of the procedure, the Contracting Party will extend the time limit for submission of tenders.

Is:

**16. Final provisions**

16. The Contracting Party reserves the right to invalidate this request for proposal at any time without providing relevant grounds therefore.

16.2 The Contracting Party may at any time cancel, amend or modify the contents of this request for proposal for convenience. If the amendments or modifications affect the contents of the tenders submitted in the course of the procedure, the Contracting Party will extend the time limit for submission of tenders.

16.3 Due to the limited functionality of the portal:

<https://bazakonkurencyjnosci.funduszeeuropejskie.gov.pl/>

The Ordering Party will publish all changes to the Inquiry documentation and the current, current state of the Inquiry documentation on the website

<https://vigo.com.pl/o-nas/zamowienia/?vigoPublicOrder=25942>

The Ordering Party has created an Inquiry with the same title and number.